Rotate servo motor

Read distance

If echo received?

Read echo signal pin

Send trigger signal continuosly

Initialize sensor

Initialize servo motor

no

yes